                    Lid cooled cavity

Symmetrical supply system

                                                                                             Lid cooled cavity

                                                                   Sketch of the flow system
water

  water at

T=T
h
y
r

m etal  pl ate at  T=T
c

                                                                                                 Geometry tested

                       (a)           (b)      (c)

(a)- cylindrical  and  (b) - cube shaped  glass cavity;

                                                (c) - cube shaped plexiglass cavity

3rd European Fluid Mechanics Conference, 15-18 Sept. 1997, Göttingen

                       Flow and Shape Instabilities of Freezing  in a

Lid Cooled Cavity

                                                                                           T.A. Kowalewski,  A. Cybulski

                                                   Polish Academy of Sciences,  IPPT PAN, Warszawa

W.J. Hiller

                                       Max-Planck-Institut für Strömungsforschung, Göttingen

                                                                                           G. de Vahl Davis, E. Leonardi

                                                                       The University of New South Wales, Sydney

Acknowledgement

                                          G. Yeoh, St. Koch, C. Abegg, C. Söller, M. Rebow